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NOTIFICATION
Corrigendum
The following communication, dated 27 July 2026, is being circulated at the request of the delegation of Rwanda.

_______________

DRS 607-1:2025, Gully tops and manhole tops for vehicular and pedestrian areas — Specification — Part 1: Classification, general design and performance requirements.
	Reason for corrigendum:

	[ ]
	Notification circulated in error

	[X]
	Clerical error in notification

	[ ]
	Clerical error in notified measure/reference document

	[ ]
	Other



Description: 

The right scope of the notified document for clarity:
This Draft Rwanda Standard specifies classification, general design, performance requirements and test methods for gully tops and manhole tops.
It applies for manhole tops and gully tops with a clear opening up to and including 1 000 mm for installation within areas subjected to pedestrian and/or vehicular traffic.
This standard is not applicable to gratings as part of prefabricated drainage channels, floor and roof gullies in buildings and surface boxes.
NOTE This Part 1 of DRS 607 is not applicable in isolation, but only in combination with DRS 607-2, DRS 607-3, DRS 607-4, DRS 607-5 and DRS 607-6.
The correct notified document is contained in:
https://members.wto.org/crnattachments/2026/TBT/RWA/26_03917_00_e.pdf
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