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NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: BOTSWANA
If applicable, name of local government involved (Articles 3.2 and 7.2): 

	2.
	Agency responsible: 
Botswana Bureau of Standards
National Enquiry Point
Botswana Bureau of Standards
Private Bag BO 48
GABORONE
Botswana
Tel: (+267) 3903200
Fax: (+267) 3903120
Toll Free Number: (0800 600 900)
Email: enquiries@bobstandards.bw

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], Other: 

	4.
	Products covered (HS codes or national tariff lines. ICS numbers may be provided in addition, where applicable): Plastics Pipes and Accessories

	5.
	Details of notified document(s) (title, number of pages and languages, means of access): BOS 78:2013 Unplasticized polyvinyl chloride (PVC-U) soil, waste and vent pipes and pipe fittings — Specification; (40 page(s), in English)
Link to notified document(s) and/or contact details for agency or authority which can provide copies upon request: 
Botswana Bureau of Standards
National Enquiry Point
Botswana Bureau of Standards
Private Bag BO 48
GABORONE
Botswana
Tel: (+267) 3903200
Fax: (+267) 3903120
Toll Free Number: (0800 600 900)
Email: enquiries@bobstandards.bw

	6.
	Description of content: This Botswana Standard specifies requirements for unplasticized poly vinyl chloride (PVC-U) pipes (including vent pipes) and pipe fittings of nominal sizes 40 mm to 160 mm intended for above-ground non-pressure applications for the conveyance of soil (human excrement or faeces) and waste water where continuous temperatures in excess of 60 °C are not encountered.
The standard specifies requirements for fittings manufactured predominantly by the injection-moulding process but does not cover fittings produced by fabrication.
The standard also gives guidance on jointing of pipes by means of solvent cement and by means of rubber joint rings.

	7.
	Objective and rationale, including the nature of urgent problems where applicable: National security requirements; Consumer information, labelling; Prevention of deceptive practices and consumer protection; Protection of human health or safety; Protection of animal or plant life or health; Protection of the environment; Quality requirements; Reducing trade barriers and facilitating trade

	8.
	Relevant documents: 
BOS ISO 4633, Rubber seals – Joint rings for water supply, drainage and sewerage pipelines – Specification for materials.

	9.
	Proposed date of adoption: Six months
Proposed date of entry into force: 6 months from adoption

	10.
	Provision of comments
Final date for comments: 14 November 2026
[X] 60 days from notification 
Contact details of agency or authority designated to handle comments regarding the notification: 
Botswana Bureau of Standards
Nametso Moilwa
Senior Documentation and Information Officer
Physical address:
Plot no: 55745
Block 8. Airport Road.
Postal address:
Botswana Bureau of Standards
Private Bag BO48
Gaborone
Tel: +267 3903200/3645604
Fax: +(267) 390 3120
Email: enquiries@bobstandards.bw; moilwa@bobstandards.bw
Website: http://www.bobstandards.bw
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