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NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: RWANDA
If applicable, name of local government involved (Articles 3.2 and 7.2): 

	2.
	Agency responsible: 
Rwanda Standards Board (RSB)
KK 15 Rd, 49
P.O.BOX 7099, Kigali, Rwanda
Tel: +250 788303492
Email: info@rsb.gov.rw
Website: www.rsb.gov.rw

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], Other: 

	4.
	Products covered (HS codes or national tariff lines. ICS numbers may be provided in addition, where applicable): Water supply systems (ICS code(s): 91.140.60)

	5.
	Details of notified document(s) (title, number of pages and languages, means of access): DRS 644-6: 2026, Plumbing works — Code of practice — Part 6: Fuel gas piping and firestop protection; (47 page(s), in English)
Link to notified document(s) and/or contact details for agency or authority which can provide copies upon request: 
https://members.wto.org/crnattachments/2026/TBT/RWA/26_03956_00_e.pdf
Rwanda Standards Board (RSB)
KK 15 Rd, 49
P.O.BOX 7099, Kigali, Rwanda
Tel: +250 788303492
Email: info@rsb.gov.rw
Website: www.rsb.gov.rw

	6.
	Description of content: 1.1 This Draft Rwanda Standard provides recommendations and guidelines for fuel gas piping and firestop protection.
1.2 Coverage of piping systems extends from the point of delivery to the appliance connections.
1.3 Fuel gas piping systems do not apply to the following items:
a) Portable LP-Gas appliances and equipment of all types that are not connected to a fixed fuel piping system.
b) Installation of appliances such as brooders, dehydrators, dryers, and irrigation equipment used for agricultural purposes.
c) Raw material (feedstock) applications except for piping to special atmosphere generators.
d) Oxygen-fuel gas cutting and welding systems.
e) Industrial gas applications using such gases as acetylene and acetylenic compounds, hydrogen, ammonia, carbon monoxide, oxygen, and nitrogen.
f) Petroleum refineries, pipeline compressor or pumping stations, loading terminals, compounding plants, refinery tank farms, and natural gas processing plants.
g) Large integrated chemical plants or portions of such plants where flammable or combustible liquids or gases are produced by chemical reactions or used in chemical reactions.
h) LP-Gas installations at utility gas plants.
i) Liquefied natural gas (LNG) installations.
j) Fuel gas piping in electric utility power plants.
k) Proprietary items of equipment, apparatus, or instruments such as gas-generating sets, compressors, and calorimeters.
l) LP-Gas equipment for vaporization, gas mixing, and gas manufacturing.
m) LP-Gas piping for buildings under construction or renovations that is not to become part of the permanent building piping system—that is, temporary fixed piping for building heat.
n) Installation of LP-Gas systems for railroad switch heating.
o) Installation of LP-Gas and compressed natural gas (CNG) systems on vehicles.
p) Gas piping, meters, gas pressure regulators, and other appurtenances used by the serving gas supplier in distribution of gas, other than undiluted LP-Gas.
q) Building design and construction, except as specified herein.
r) Fuel gas systems on recreational vehicles manufactured in accordance with national standards in place on fire and health safety criteria for recreational vehicles.
s) Fuel gas systems using hydrogen as a fuel.
t) Construction of appliances.
1.4 Firestop protection systems include piping penetrations of required fire-resistance-rated walls, partitions, floors, floor/ceiling assemblies, roof/ceiling assemblies, or shaft enclosures are to be protected in accordance with the requirements of the Rwanda building code.

	7.
	Objective and rationale, including the nature of urgent problems where applicable: Consumer information, labelling; Prevention of deceptive practices and consumer protection; Protection of human health or safety; Protection of the environment; Quality requirements; Reducing trade barriers and facilitating trade; Cost saving and productivity enhancement

	8.
	Relevant documents: 
1. ASTM A53, Standard Specification for Pipe, Steel, Black and Hot-Dipped, Zinc-Coated, Welded and Seamless
2. ASTM A106, Standard Specification for Seamless Carbon Steel Pipe for High-Temperature Service
3. ASTM A312, Standard Specification for Seamless, Welded, and Heavily Cold Worked Austenitic Stainless Steel Pipes
4. ASTM A268, Standard Specification for Seamless and Welded Ferritic and Martensitic Stainless Steel Tubing for General Service
5. ASTM A269, Standard Specification for Seamless and Welded Austenitic Stainless Steel Tubing for General Service
6. ASTM B88, Standard Specification for Seamless Copper Water Tube
7. ASTM B280, Standard Specification for Seamless Copper Tube for Air Conditioning and Refrigeration Field Service
8. ASTM B210, Standard Specification for Aluminum and Aluminum-Alloy Drawn Seamless Tubes
9. ASTM B241, Standard Specification for Aluminum and Aluminum-Alloy Seamless Pipe and Seamless Extruded Tube
10. ASTM D2513, Standard Specification for Polyethylene (PE) Gas Pressure Pipe, Tubing, and Fittings
11. ASTM F2945, Standard Specification for Polyamide 11 Gas Pressure Pipe, Tubing, and Fittings
12. ASTM D2513, Standard Specification for Polyethylene (PE) Gas Pressure Pipe, Tubing, and Fittings
13. ASTM F1973, Standard Specification for Factory Assembled Anodeless Risers and Transition Fittings in Polyethylene (PE) and Polyamide 11 (PA11) and Polyamide 12 (PA12) Fuel Gas Distribution Systems
14. ASTM F2509, Standard Specification for Field-assembled Anodeless Riser Kits for Use on Outside Diameter Controlled Polyethylene and Polyamide-11 (PA11) Gas Distribution Pipe and Tubing
15. UL 467, Grounding and Bonding Solutions Certification Testing

	9.
	Proposed date of adoption: To be determined
Proposed date of entry into force: 6 months from adoption

	10.
	Provision of comments
Final date for comments: 26 September 2026
[X] 60 days from notification 
Contact details of agency or authority designated to handle comments regarding the notification: 
Rwanda Standards Board (RSB)
KK 15 Rd, 49
P.O.BOX 7099, Kigali, Rwanda
Tel: +250 788303492
Email: info@rsb.gov.rw
Website: www.rsb.gov.rw
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